

Fibre channel SAN- every computer is connected to a SAN switch to an external RAID device.

iSCSI SAN- Ethernet switch connected to computer through fiber optic to a raid



Cluster in a SAN- the users are a signal device and can replace any device that fails